**NextEngine 3D scanner**

Software on desktop – Scanstudio

Set Platform Within image window  
Start

Scan types

* 360 = full coverage
* Bracket = Specify Coverage
* Frontal = front plane

export as STL  
compare generated STL to supplied STL